|  |  |
| --- | --- |
| Fuel Composition  [% vol] | Lower heating value  [MJ/kmol] |
| Methane | 800 |
| Hydrogen/methane 50%/50% | 520 |
| Hydrogen | 240 |
| Hydrogen/nitrogen 85%/15% | 204 |